import processing.serial.\*;

import java.awt.event.KeyEvent;

import java.io.IOException;

Serial myPort;// defubes variables

String distance="";

String data="";

String noObject;

String angle="";

float pixsDistance;

int iAngle, iDistance;

int index1=0;

int index2=0;

PFont orcFont;

void setup() {

size (1280 ,720);

smooth();

myPort = new Serial(this,"COM3", 9600); // change this accordingly

myPort.bufferUntil('.'); // reads the data from the serial port up to the character ‘.’. So actually it reads this: angle,distance.

}

void draw() {

fill(98,245,31);

// simulating motion blur and slow fade of the moving line

noStroke();

fill(0,4);

rect(0, 0, width, height-height\*0.065);

fill(98,245,31); // green color

// calls the functions for drawing the radar

drawRadar();

drawLine();

drawObject();

drawText();

}

void serialEvent (Serial myPort) { // starts reading data from the Serial Port

// reads the data from the Serial Port up to the character ‘.’ and puts it into the String variable “data”.

data = myPort.readStringUntil('.');

data = data.substring(0,data.length()-1);

index1 = data.indexOf(','); // find the character ‘,’ and puts it into the variable “index1”

angle= data.substring(0, index1); // read the data from position “0” to position of the variable index1 or thats the value of the angle the Arduino Board sent into the Serial Port

distance= data.substring(index1+1, data.length()); // read the data from position “index1” to the end of the data pr thats the value of the distance

// converts the String variables into Integer

iAngle = int(angle);

iDistance = int(distance);

}

void drawRadar() {

pushMatrix();

translate(width/2,height-height\*0.074); // moves the starting coordinats to new location

noFill();

strokeWeight(2);

stroke(98,245,31);

// draws the arc lines

arc(0,0,(width-width\*0.0625),(width-width\*0.0625),PI,TWO\_PI);

arc(0,0,(width-width\*0.27),(width-width\*0.27),PI,TWO\_PI);

arc(0,0,(width-width\*0.479),(width-width\*0.479),PI,TWO\_PI);

arc(0,0,(width-width\*0.687),(width-width\*0.687),PI,TWO\_PI);

// draws the angle lines

line(-width/2,0,width/2,0);

line(0,0,(-width/2)\*cos(radians(30)),(-width/2)\*sin(radians(30)));

line(0,0,(-width/2)\*cos(radians(60)),(-width/2)\*sin(radians(60)));

line(0,0,(-width/2)\*cos(radians(90)),(-width/2)\*sin(radians(90)));

line(0,0,(-width/2)\*cos(radians(120)),(-width/2)\*sin(radians(120)));

line(0,0,(-width/2)\*cos(radians(150)),(-width/2)\*sin(radians(150)));

line((-width/2)\*cos(radians(30)),0,width/2,0);

popMatrix();

}

void drawObject() {

pushMatrix();

translate(width/2,height-height\*0.074); // moves the starting coordinats to new location

strokeWeight(9);

stroke(255,10,10); // red color

pixsDistance = iDistance\*((height-height\*0.1666)\*0.025); // covers the distance from the sensor from cm to pixels

// limiting the range to 40 cms

if(iDistance<40){

// draws the object according to the angle and the distance

line(pixsDistance\*cos(radians(iAngle)),-pixsDistance\*sin(radians(iAngle)),(width-width\*0.505)\*cos(radians(iAngle)),-(width-width\*0.505)\*sin(radians(iAngle)));

}

popMatrix();

}

void drawLine() {

pushMatrix();

strokeWeight(9);

stroke(30,250,60);

translate(width/2,height-height\*0.074); // moves the starting coordinats to new location

line(0,0,(height-height\*0.12)\*cos(radians(iAngle)),-(height-height\*0.12)\*sin(radians(iAngle))); // draws the line according to the angle

popMatrix();

}

void drawText() { // draws the texts on the screen

pushMatrix();

if(iDistance>40) {

noObject = "Out of Range";

}

else {

noObject = "In Range";

}

fill(0,0,0);

noStroke();

rect(0, height-height\*0.0648, width, height);

fill(98,245,31);

textSize(25);

text("10cm",width-width\*0.3854,height-height\*0.0833);

text("20cm",width-width\*0.281,height-height\*0.0833);

text("30cm",width-width\*0.177,height-height\*0.0833);

text("40cm",width-width\*0.0729,height-height\*0.0833);

textSize(40);

text("Radar Graph", width-width\*0.875, height-height\*0.0277);

text("Angle: " + iAngle +" °", width-width\*0.48, height-height\*0.0277);

text("", width-width\*0.26, height-height\*0.0277);

if(iDistance<40) {

text(" " + iDistance +" cm", width-width\*0.225, height-height\*0.0277);

}

textSize(25);

fill(98,245,60);

translate((width-width\*0.4994)+width/2\*cos(radians(30)),(height-height\*0.0907)-width/2\*sin(radians(30)));

rotate(-radians(-60));

text("30°",0,0);

resetMatrix();

translate((width-width\*0.503)+width/2\*cos(radians(60)),(height-height\*0.0888)-width/2\*sin(radians(60)));

rotate(-radians(-30));

text("60°",0,0);

resetMatrix();

translate((width-width\*0.507)+width/2\*cos(radians(90)),(height-height\*0.0833)-width/2\*sin(radians(90)));

rotate(radians(0));

text("90°",0,0);

resetMatrix();

translate(width-width\*0.513+width/2\*cos(radians(120)),(height-height\*0.07129)-width/2\*sin(radians(120)));

rotate(radians(-30));

text("120°",0,0);

resetMatrix();

translate((width-width\*0.5104)+width/2\*cos(radians(150)),(height-height\*0.0574)-width/2\*sin(radians(150)));

rotate(radians(-60));

text("150°",0,0);

popMatrix();

}